Building configuration...

Current configuration : 1834 bytes

!

! Last configuration change at 03:29:24 UTC Mon Mar 1 1993

!

version 15.0

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname S2

!

boot-start-marker

boot-end-marker

!

no aaa new-model

system mtu routing 1500

!

spanning-tree mode pvst

spanning-tree extend system-id

!

vlan internal allocation policy ascending

!

interface Port-channel1

switchport trunk allowed vlan 10,20,30

switchport mode trunk

!

interface FastEthernet0/1

!

interface FastEthernet0/2

switchport access vlan 10

switchport mode access

!

interface FastEthernet0/3

switchport access vlan 20

switchport mode access

!

interface FastEthernet0/4

switchport access vlan 30

switchport mode access

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

switchport trunk allowed vlan 10,20,30

switchport mode trunk

channel-protocol lacp

channel-group 1 mode active

!

interface FastEthernet0/24

switchport trunk allowed vlan 10,20,30

switchport mode trunk

channel-protocol lacp

channel-group 1 mode active

!

interface GigabitEthernet0/1

switchport mode trunk

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

!

interface Vlan30

ip address 192.168.25.254 255.255.255.0

!

ip http server

ip http secure-server

!

line con 0

line vty 5 15

!

end