Building configuration...

Current configuration : 1857 bytes

!

! Last configuration change at 11:52:37 UTC Wed May 24 2017

version 15.3

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname R2

!

boot-start-marker

boot-end-marker

!

no aaa new-model

!

ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

license udi pid CISCO2901/K9 sn FCZ1850C2MS

license boot module c2900 technology-package securityk9

license boot module c2900 technology-package datak9

!

redundancy

!

interface Embedded-Service-Engine0/0

no ip address

shutdown

!

interface GigabitEthernet0/0

no ip address

duplex auto

speed auto

!

interface GigabitEthernet0/0.10

encapsulation dot1Q 10

ip address 192.168.5.1 255.255.255.0

standby 1 ip 192.168.5.10

!

interface GigabitEthernet0/0.20

encapsulation dot1Q 20

ip address 192.168.15.1 255.255.255.0

standby 2 ip 192.168.15.10

!

interface GigabitEthernet0/0.30

encapsulation dot1Q 30

ip address 192.168.25.1 255.255.255.0

standby 3 ip 192.168.25.10

!

interface GigabitEthernet0/1

ip address 10.10.10.2 255.255.255.0

duplex auto

speed auto

!

interface GigabitEthernet0/1.10

!

interface Serial0/0/0

ip address 172.16.15.2 255.255.255.252

!

interface Serial0/0/1

no ip address

shutdown

clock rate 2000000

!

router ospf 10

network 10.10.10.0 0.0.0.255 area 0

network 172.16.15.0 0.0.0.3 area 0

network 192.168.25.0 0.0.0.255 area 0

!

ip forward-protocol nd

!

no ip http server

no ip http secure-server

!

ip route 0.0.0.0 0.0.0.0 172.16.25.1

ip route 0.0.0.0 0.0.0.0 172.16.15.1

!

control-plane

!

line con 0

line aux 0

line 2

no activation-character

no exec

transport preferred none

transport output lat pad telnet rlogin lapb-ta mop udptn v120 ssh

stopbits 1

line vty 0 4

login

transport input all

!

scheduler allocate 20000 1000

!

end